{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["port"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"port","index":0,"n_rows":198,"n_cols":9,"rows_kept":198,"cut":false,"hidden":false,"merged":[[187,2,187,3],[188,2,188,3]],"flags":["formulas_cached_only"]}
[]
[null,null,"GPIO","機能１","機能２","機能３","機能1/2/3の選択","備考","GPIO使用可"]
[null,"PTA7"," 入出力"," D23 入出力 (BSC)"," KEYOUT2 出力 (KEYSC)"," IDED15 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-18A",1]
[null,"PTA6"," 入出力"," D22 入出力 (BSC)"," KEYOUT1 出力 (KEYSC)"," IDED14 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-18B",1]
[null,"PTA5"," 入出力"," D21 入出力 (BSC)"," KEYOUT0 出力 (KEYSC)"," IDED13 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-19A",1]
[null,"PTA4"," 入出力"," D20 入出力 (BSC)"," KEYIN4 入力 (KEYSC)"," IDED12 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-19B",1]
[null,"PTA3"," 入出力"," D19 入出力 (BSC)"," KEYIN3 入力 (KEYSC)"," IDED11 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-20A",1]
[null,"PTA2"," 入出力"," D18 入出力 (BSC)"," KEYIN2 入力 (KEYSC)"," IDED10 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-20B",1]
[null,"PTA1"," 入出力"," D17 入出力 (BSC)"," KEYIN1 入力 (KEYSC)"," IDED9 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-21A",1]
[null,"PTA0"," 入出力"," D16 入出力 (BSC)"," KEYIN0 入力 (KEYSC)"," IDED8 入出力 (ATAPI)","PSA[15:14]","EB724 CN7-21B",1]
[null,"PTB7"," 入出力"," D31 入出力 (BSC)"," TPUTO1 出力 (TPU)"," IDEA1 出力 (ATAPI)","PSE[15:14]","EB724 CN7-16A",2]
[null,"PTB6"," 入出力"," D30 入出力 (BSC)"," TPUTO0 出力 (TPU)"," IDEA0 出力 (ATAPI)","PSE[15:14]","EB724 CN7-16B",2]
[null,"PTB5"," 入出力"," D29 入出力 (BSC)"," － ","IODREQ 入力 (ATAPI)","PSE[11]","EB724ではDIPSW4",4]
[null,"PTB4"," 入出力"," D28 入出力 (BSC)"," － ","IDECS0 出力 (ATAPI)","PSE[11]","EB724ではDIPSW3",4]
[null,"PTB3"," 入出力"," D27 入出力 (BSC)"," － ","IDECS1 出力 (ATAPI)","PSE[11]","EB724ではDIPSW2",4]
[null,"PTB2"," 入出力"," D26 入出力 (BSC)"," KEYOUT5/IN5 入出力 (KEYSC)"," IDEIORD 出力 (ATAPI)","PSA[15:14]","EB724ではDIPSW1",4]
[null,"PTB1"," 入出力"," D25 入出力 (BSC)"," KEYOUT4/IN6 入出力 (KEYSC)"," IDEIOWR 出力 (ATAPI)","PSA[15:14]","EB724 CN7-17A",1]
[null,"PTB0"," 入出力"," D24 入出力 (BSC)"," KEYOUT3 出力 (KEYSC)"," IDEINT 入力 (ATAPI)","PSA[15:14]","EB724 CN7-17B",1]
[null,"PTC7"," 入出力"," LCDD7 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTC6"," 入出力"," LCDD6 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTC5"," 入出力"," LCDD5 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTC4"," 入出力"," LCDD4 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTC3"," 入出力"," LCDD3 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTC2"," 入出力"," LCDD2 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTC1"," 入出力"," LCDD1 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTC0"," 入出力"," LCDD0 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD7"," 入出力"," LCDD15 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD6"," 入出力"," LCDD14 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD5"," 入出力"," LCDD13 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD4"," 入出力"," LCDD12 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD3"," 入出力"," LCDD11 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD2"," 入出力"," LCDD10 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD1"," 入出力"," LCDD9 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTD0"," 入出力"," LCDD8 入出力 (LCDC)"," －"," －","PSD[5]","EB724ではLCD",4]
[null,"PTE7"," 入出力"," FSIMCKB 入力 (FSI)"," －"," －"," －","EB724 CN2-17B",1]
[null,"PTE6"," 入出力"," FSIMCKA 入力 (FSI)"," －"," －"," －","EB724ではAudio Clock 入力",4]
[null,"PTE5"," 入出力 (PullDown)"," LCDD21 入出力 (LCDC)"," SCIF2_TXD 出力 (SCIF2)"," －","PSC[5:4]/MSELB[7]","EB724 CN2-3B",2]
[null,"PTE4"," 入出力 (PullDown)"," LCDD20 入出力 (LCDC)"," SCIF4_SCK 入出力 (SCIFA4)"," －","PSD[3:2]","EB724では未接続",3]
[null,"PTE3"," 入出力 (PullDown)"," LCDD19 入出力 (LCDC)"," SCIF4_RXD 入力 (SCIFA4)"," －","PSA[3:2]","EB724 CN2-4A",2]
[null,"PTE2"," 入出力 (PullDown)"," LCDD18 入出力 (LCDC)"," SCIF4_TXD 出力 (SCIFA4)"," －","PSA[3:2]","EB724 CN2-4B",2]
[null,"PTE1"," 入出力 (PullDown)"," LCDD17 入出力 (LCDC)"," －"," －","PSD[6]","EB724ではLCD",4]
[null,"PTE0"," 入出力 (PullDown)"," LCDD16 入出力 (LCDC)"," －"," －","PSD[6]","EB724ではLCD",4]
[null,"PTF7"," 入出力"," LCDVSYN 入出力 (LCDC)"," －"," －","PSD[8]","EB724ではLCD",4]
[null,"PTF6"," 入出力"," LCDDISP/LCDRS 出力 (LCDC)"," －"," －","PSD[10:9]","EB724ではLCD",4]
[null,"PTF5"," 入出力"," LCDHSYN/LCDCS 出力 (LCDC)"," －"," －","PSD[10:9]","EB724ではLCD",4]
[null,"PTF4"," 入出力"," LCDDON 出力 (LCDC)"," －"," －","PSD[8]","EB724では未接続",3]
[null,"PTF3"," 入出力"," LCDDCK/LCDWR 出力 (LCDC)"," －"," －","PSD[10:9]","EB724ではLCD",4]
[null,"PTF2"," 入出力"," LCDVEPWC 出力 (LCDC)"," SCIF0_TXD 出力 (SCIF0)"," －","PSA[6]","コンソールとして使用"]
[null,"PTF1"," 入出力"," LCDD23 入出力 (LCDC)"," SCIF2_SCK 入出力 (SCIF2)"," －","PSC[7:6]/MSELB[7]","EB724では未接続",3]
[null,"PTF0"," 入出力"," LCDD22 入出力 (LCDC)"," SCIF2_RXD 入力 (SCIF2)"," －","PSC[5:4]/MSELB[7]","EB724 CN2-3A",2]
[null,"PTG7"," －"," －"," －"," －"," －","n.c."]
[null,"PTG6"," －"," －"," －"," －"," －","n.c."]
[null,"PTG5"," 出力"," AUDCK 出力 (AUD)"," －"," －"," －","EB724では未接続",3]
[null,"PTG4"," 出力"," AUDSYNC 出力 (AUD)"," －"," －"," －","EB724では未接続",3]
[null,"PTG3"," 出力"," AUDATA3 出力 (AUD)"," －"," －"," －","EB724ではLED4",4]
[null,"PTG2"," 出力"," AUDATA2 出力 (AUD)"," －"," －"," －","EB724ではLED3",4]
[null,"PTG1"," 出力"," AUDATA1 出力 (AUD)"," －"," －"," －","EB724ではLED2",4]
[null,"PTG0"," 出力"," AUDATA0 出力 (AUD)"," －"," －"," －","EB724ではLED1",4]
[null,"PTH7"," 入出力"," VIO0_VD 入力 (VIO)"," －"," －"," －","EB724 CN7-9A",1]
[null,"PTH6"," 入出力"," VIO0_CLK 入力 (VIO)"," －"," －"," －","EB724 CN7-9B",1]
[null,"PTH5"," 入出力"," VIO0_D7 入力 (VIO)"," －"," －"," －","EB724 CN7-10A",1]
[null,"PTH4"," 入出力"," VIO0_D6 入力 (VIO)"," －"," －"," －","EB724 CN7-10B",1]
[null,"PTH3"," 入出力"," VIO0_D5 入力 (VIO)"," －"," －"," －","EB724 CN7-11A",1]
[null,"PTH2"," 入出力"," VIO0_D4 入力 (VIO)"," －"," －"," －","EB724 CN7-11B",1]
[null,"PTH1"," 入出力"," VIO0_D3 入力 (VIO)"," －"," －"," －","EB724 CN7-12A",1]
[null,"PTH0"," 入出力"," VIO0_D2 入力 (VIO)"," －"," －"," －","EB724 CN7-12B",1]
[null,"PTJ7"," 出力"," PDSTATUS 出力 (システム)"," －"," －"," －","CAT724 LED2"]
[null,"PTJ6"," 出力"," STATUS2 出力 (システム)"," －"," －"," －","CAT724 LED1"]
[null,"PTJ5"," 出力"," STATUS0 出力 (システム)"," －"," －"," －","n.c."]
[null,"PTJ4"," －"," －"," －"," －"," －","n.c."]
[null,"PTJ3"," 入出力"," A25 出力 (BSC)"," BS 出力 (BSC)"," －","PSA[8]"]
[null,"PTJ2"," 入出力"," A24 出力 (BSC)"," －"," －"," －"]
[null,"PTJ1"," 入出力"," A23 出力 (BSC)"," －"," －"," －"]
[null,"PTJ0"," 入出力"," A22 出力 (BSC)"," －"," －"," －"]
[null,"PTK7"," 入出力"," VIO1_D5 入力 (VIO)"," VIO0_D13 入力 (VIO)"," IDED5 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTK6"," 入出力"," VIO1_D4 入力 (VIO)"," VIO0_D12 入力 (VIO)"," IDED4 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTK5"," 入出力"," VIO1_D3 入力 (VIO)"," VIO0_D11 入力 (VIO)"," IDED3 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTK4"," 入出力"," VIO1_D2 入力 (VIO)"," VIO0_D10 入力 (VIO)"," IDED2 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTK3"," 入出力"," VIO1_D1 入力 (VIO)"," VIO0_D9 入力 (VIO)"," IDED1 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTK2"," 入出力"," VIO1_D0 入力 (VIO)"," VIO0_D8 入力 (VIO)"," IDED0 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTK1"," 入出力"," VIO0_FLD 入力 (VIO)"," －"," －"," －","EB724 CN2-8A",1]
[null,"PTK0"," 入出力"," VIO0_HD 入力 (VIO)"," －"," －"," －","EB724 CN2-8B",1]
[null,"PTL7"," 入出力"," DV_D5 出力 (VOU)"," SCIF3_SCK 入出力 (SCIFA3)"," RMII_RXD0 入力 (EtherMAC)","PSB[9:8]/MSELB[5]","EB724 CN2-9A",1]
[null,"PTL6"," 入出力"," DV_D4 出力 (VOU)"," SCIF3_RXD 入力 (SCIFA3)"," RMII_RXD1 入力 (EtherMAC)","PSB[9:8]/MSELB[5]","EB724 CN2-9B",2]
[null,"PTL5"," 入出力"," DV_D3 出力 (VOU)"," SCIF3_TXD 出力 (SCIFA3)"," RMII_REF_CLK 入力 (EtherMAC)","PSE[7:6]/MSELB[5]","EB724 CN2-10A",2]
[null,"PTL4"," 入出力"," DV_D2 出力 (VOU)"," SCIF1_SCK 入出力 (SCIF1)"," RMII_TX_EN 出力 (EtherMAC)","PSC[9:8]","EB724 CN2-10B",1]
[null,"PTL3"," 入出力"," DV_D1 出力 (VOU)"," SCIF1_RXD 入力 (SCIF1)"," RMII_TXD0 出力 (EtherMAC)","PSC[9:8]","EB724 CN2-11A",2]
[null,"PTL2"," 入出力"," DV_D0 出力 (VOU)"," SCIF1_TXD 出力 (SCIF1)"," RMII_TXD1 出力 (EtherMAC)","PSC[9:8]","EB724 CN2-11B",2]
[null,"PTL1"," 入出力"," DV_D15 出力 (VOU)"," －"," －","PSD[4]","EB724 CN2-12A",1]
[null,"PTL0"," 入出力"," DV_D14 出力 (VOU)"," MSIOF0_MCK  入出力 (MSIOF0)"," －","PSE[5:4]","EB724 CN2-12B",1]
[null,"PTM7"," 入出力"," DV_D13 出力 (VOU)"," MSIOF0_TSCK 入出力 (MSIOF0)"," －","PSC[13:12]","EB724 CN2-13A",1]
[null,"PTM6"," 入出力"," DV_D12 出力 (VOU)"," MSIOF0_RXD 入力 (MSIOF0)"," －","PSC[13:12]","EB724 CN2-13B",1]
[null,"PTM5"," 入出力"," DV_D11 出力 (VOU)"," MSIOF0_TXD 出力 (MSIOF0)"," －","PSC[13:12]","EB724 CN2-14A",1]
[null,"PTM4"," 入出力"," DV_D10 出力 (VOU)"," MSIOF0_TSYNC 入出力 (MSIOF0)"," －","PSC[13:12]","EB724 CN2-14B",1]
[null,"PTM3"," 入出力"," DV_D9 出力 (VOU)"," MSIOF0_SS1/MSIOF0_RSCK 入出力 (MSIOF0)"," －","PSC[11:10]","EB724 CN2-15A",1]
[null,"PTM2"," 入出力"," DV_D8 出力 (VOU)"," MSIOF0_SS2/MSIOF0_RSYNC 入出力 (MSIOF0)"," －","PSC[11:10]","EB724 CN2-15B",1]
[null,"PTM1"," 入出力"," LCDVCPWC 出力 (LCDC)"," SCIF0_RXD 入力 (SCIF0)"," －","PSA[6]","コンソールとして使用"]
[null,"PTM0"," 入出力"," LCDRD 出力 (LCDC)"," SCIF0_SCK 入出力 (SCIF0)"," －","PSA[7]","EB724 SDソケット電源制御",4]
[null,"PTN7"," 入出力"," VIO0_D1 入力 (VIO)"," －"," －"," －","EB724 CN2-13A",1]
[null,"PTN6"," 入出力"," VIO0_D0 入力 (VIO)"," －"," －"," －","EB724 CN2-13B",1]
[null,"PTN5"," 入出力 (PullDown)"," DV_CLKI 入力 (VOU)"," －"," －","PSD[11]","EB724 CN7-6A",1]
[null,"PTN4"," 入出力"," DV_CLK 出力 (VOU)"," SCIF2_SCK 入出力 (SCIF2)"," －","PSD[13:12]/MSELB[7]","EB724 CN7-6B",1]
[null,"PTN3"," 入出力"," DV_VSYNC 出力 (VOU)"," SCIF2_RXD 入力 (SCIF2)"," －","PSD[15:14]/MSELB[7]","EB724 CN7-7A",2]
[null,"PTN2"," 入出力"," DV_HSYNC 出力 (VOU)"," SCIF2_TXD 出力 (SCIF2)"," －","PSB[5:4]/MSELB[7]","EB724 CN7-7B",2]
[null,"PTN1"," 入出力"," DV_D7 出力 (VOU)"," SCIF3_CTS 入力 (SCIFA3)"," RMII_RX_ER 入力 (EtherMAC)","PSB[3:2]/MSELB[5]","EB724 CN7-8A",1]
[null,"PTN0"," 入出力"," DV_D6 出力 (VOU)"," SCIF3_RTS 出力 (SCIFA3)"," RMII_CRS_DV 入力 (EtherMAC)","PSB[1:0]/MSELB[5]","EB724 CN7-8B",1]
[null,"PTQ7"," 入出力 (PullDown)"," D7 入出力 (BSC)"," －"," －"," －"]
[null,"PTQ6"," 入出力 (PullDown)"," D6 入出力 (BSC)"," －"," －"," －"]
[null,"PTQ5"," 入出力 (PullDown)"," D5 入出力 (BSC)"," －"," －"," －"]
[null,"PTQ4"," 入出力 (PullDown)"," D4 入出力 (BSC)"," －"," －"," －"]
[null,"PTQ3"," 入出力 (PullDown)"," D3 入出力 (BSC)"," －"," －"," －"]
[null,"PTQ2"," 入出力 (PullDown)"," D2 入出力 (BSC)"," －"," －"," －"]
[null,"PTQ1"," 入出力 (PullDown)"," D1 入出力 (BSC)"," －"," －"," －"]
[null,"PTQ0"," 入出力 (PullDown)"," D0 入出力 (BSC)"," －"," －"," －"]
[null,"PTR7"," 入出力"," CS6B/CE1B 出力 (BSC)"," －"," －"," －"]
[null,"PTR6"," 入出力"," CS6A/CE2B 出力 (BSC)"," －"," －"," －"]
[null,"PTR5"," 入出力"," CS5B/CE1A 出力 (BSC)"," －"," －"," －","CAT724 DIPSW2"]
[null,"PTR4"," 入出力"," CS5A/CE2A 出力 (BSC)"," －"," －"," －","CAT724 DIPSW1"]
[null,"PTR3"," 入力"," IOIS16 入力 (BSC)"," LCDLCLK 入力 (LCDC)"," －","PSA[5]","LCDクロック外部入力（未実装）"]
[null,"PTR2"," 入力"," WAIT 入力 (BSC)"," －"," －"," －","H固定 （未使用）"]
[null,"PTR1"," 入出力"," WE3/ICIOWR 出力 (BSC)"," TPUTO3 出力 (TPU)"," TPUTI3 入力 (TPU)","PSA[1:0]","CAT724 ソフトI2C"]
[null,"PTR0"," 入出力"," WE2/ICIORD 出力 (BSC)"," TPUTO2 出力 (TPU)"," IDEA2 出力 (ATAPI)","PSD[1:0]","CAT724 ソフトI2C"]
[null,"PTS7"," －"," －"," －"," －"," －","n.c."]
[null,"PTS6"," 入出力"," VIO_CKO 出力 (VIO)"," －"," －"," －","EB724 CN2-6A",1]
[null,"PTS5"," 入出力"," VIO1_FLD 入力 (VIO)"," TPUTI2 入力 (TPU)"," IDEIORDY 入力 (ATAPI)","PSE[9:8]","EB724 CN2-6B",1]
[null,"PTS4"," 入出力"," VIO1_HD 入力 (VIO)"," SCIF5_SCK 入出力 (SCIFA5)"," －","PSA[10]","EB724では未接続",3]
[null,"PTS3"," 入出力"," VIO1_VD 入力 (VIO)"," SCIF5_RXD 入力 (SCIFA5)"," －","PSA[9]","EB724 CN2-7A",1]
[null,"PTS2"," 入出力"," VIO1_CLK 入力 (VIO)"," SCIF5_TXD 出力 (SCIFA5)"," －","PSA[9]","EB724 CN2-7B",1]
[null,"PTS1"," 入出力"," VIO1_D7 入力 (VIO)"," VIO0_D15 入力 (VIO)"," IDED7 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTS0"," 入出力"," VIO1_D6 入力 (VIO)"," VIO0_D14 入力 (VIO)"," IDED6 入出力 (ATAPI)","PSB[7:6]","EB724では未接続",3]
[null,"PTT7"," 入出力 (PullDown)"," D15 入出力 (BSC)"," －"," －"," －"]
[null,"PTT6"," 入出力 (PullDown)"," D14 入出力 (BSC)"," －"," －"," －"]
[null,"PTT5"," 入出力 (PullDown)"," D13 入出力 (BSC)"," －"," －"," －"]
[null,"PTT4"," 入出力 (PullDown)"," D12 入出力 (BSC)"," －"," －"," －"]
[null,"PTT3"," 入出力 (PullDown)"," D11 入出力 (BSC)"," －"," －"," －"]
[null,"PTT2"," 入出力 (PullDown)"," D10 入出力 (BSC)"," －"," －"," －"]
[null,"PTT1"," 入出力 (PullDown)"," D9 入出力 (BSC)"," －"," －"," －"]
[null,"PTT0"," 入出力 (PullDown)"," D8 入出力 (BSC)"," －"," －"," －"]
[null,"PTU7"," 入出力"," DACK0 出力 (DMAC)"," －"," －"," －","CAT724 DIPSW4"]
[null,"PTU6"," 入出力"," DREQ0 入力 (DMAC)"," －"," －"," －","CAT724 DIPSW3"]
[null,"PTU5"," 入出力"," FSIOASD 出力 (FSI)"," －"," －","PSE[1]","EB724ではDATAI (Audio)",4]
[null,"PTU4"," 入出力"," FSIIABCK 入力 (FSI)"," －"," －","PSE[1]","EB724では未接続",3]
[null,"PTU3"," 入出力"," FSIIALRCK 入力 (FSI)"," －"," －","PSE[1]","EB724では未接続",3]
[null,"PTU2"," 入出力"," FSIOABCK 出力 (FSI)"," －"," －","PSE[1]","EB724ではBCK (audio)",4]
[null,"PTU1"," 入出力"," FSIOALRCK 出力 (FSI)"," －"," －","PSE[1]","EB724ではWS (audio)",4]
[null,"PTU0"," 入出力"," CLKAUDIOAO 出力 (FSI)"," －"," －","PSE[0]","EB724では未接続",3]
[null,"PTV7"," 入出力"," FSIIBSD 入力 (FSI)"," MSIOF1_SS2/MSIOF1_RSYNC 入出力 (MSIOF1)"," －","PSD[7:6]","EB724 CN2-14A",1]
[null,"PTV6"," 入出力"," FSIOBSD 出力 (FSI)"," MSIOF1_SS1/MSIOF1_RSCK 入出力 (MSIOF1)"," －","PSD[7:6]","EB724 CN2-14B",1]
[null,"PTV5"," 入出力"," FSIIBBCK 入力 (FSI)"," MSIOF1_RXD 入力 (MSIOF1)"," －","PSC[15:14]","EB724 CN2-15A",1]
[null,"PTV4"," 入出力"," FSIIBLRCK 入力 (FSI)"," MSIOF1_TSYNC 出力 (MSIOF1)"," －","PSC[15:14]","EB724 CN2-15B",1]
[null,"PTV3"," 入出力"," FSIOBBCK 出力 (FSI)"," MSIOF1_TSCK 入出力 (MSIOF1)"," －","PSC[15:14]","EB724 CN2-16A",1]
[null,"PTV2"," 入出力"," FSIOBLRCK 出力 (FSI)"," MSIOF1_TXD 出力 (MSIOF1)"," －","PSC[15:14]","EB724 CN2-16B",1]
[null,"PTV1"," 入出力"," CLKAUDIOBO 出力 (FSI)"," MSIOF1_MCK 入力 (MSIOF1)"," －","PSE[3:2]","EB724 CN2-17A",1]
[null,"PTV0"," 入出力"," FSIIASD 入力 (FSI)"," －"," －","PSE[10]","EB724では未接続",3]
[null,"PTW7"," 入出力"," MMC_D7 入出力 (MMCIF)"," SDHI1CD 入力 (SDHI1)"," IODACK 出力 (ATAPI)","PSE[13:12]","EB724ではSD",4]
[null,"PTW6"," 入出力"," MMC_D6 入出力 (MMCIF)"," SDHI1WP 入力 (SDHI1)"," IDERST 出力(ATAPI)","PSE[13:12]","EB724ではSD",4]
[null,"PTW5"," 入出力"," MMC_D5 入出力 (MMCIF)"," SDHI1D3 入出力 (SDHI1)"," EXBUF_ENB 出力 (ATAPI)","PSE[13:12]","EB724ではSD",4]
[null,"PTW4"," 入出力"," MMC_D4 入出力 (MMCIF)"," SDHI1D2 入出力 (SDHI1)"," DIRECTION 出力 (ATAPI)","PSE[13:12]","EB724ではSD",4]
[null,"PTW3"," 入出力"," MMC_D3 入出力 (MMCIF)"," SDHI1D1 入出力 (SDHI1)"," －","PSA[13]","EB724ではSD",4]
[null,"PTW2"," 入出力"," MMC_D2 入出力 (MMCIF)"," SDHI1D0 入出力 (SDHI1)"," －","PSA[13]","EB724ではSD",4]
[null,"PTW1"," 入出力"," MMC_D1 入出力 (MMCIF)"," SDHI1CMD 入出力 (SDHI1)"," －","PSA[13]","EB724ではSD",4]
[null,"PTW0"," 入出力"," MMC_D0 入出力 (MMCIF)"," SDHI1CLK 出力 (SDHI1)"," －","PSA[13]","EB724ではSD",4]
[null,"PTX7"," 入出力"," DACK1 出力 (DMAC)"," IRDA_OUT 出力 (IrDA)"," －","PSA[12]","USB1 Enable"]
[null,"PTX6"," 入出力"," DREQ1 入力 (DMAC)"," IRDA_IN 入力 (IrDA)"," －","PSA[12]","USB1 OverCurrent"]
[null,"PTX5"," 入出力 (PullDown)"," TS0_SDAT 入力 (TSIF)"," －"," LNKSTA 入力 (EtherMAC)","PSC[0]","EB724 CN7-4A",1]
[null,"PTX4"," 入出力 (PullDown)"," TS0_SCK 入力 (TSIF)"," －"," MDIO 入出力 (EtherMAC)","PSC[1]","EB724 CN7-4B",1]
[null,"PTX3"," 入出力 (PullDown)"," TS0_SDEN 入力 (TSIF)"," －"," MDC 出力 (EtherMAC)","PSC[2]","EB724 CN7-5A",1]
[null,"PTX2"," 入出力 (PullDown)"," TS0_SPSYNC 入力 (TSIF)"," －"," －"," －","EB724 CN7-5B",1]
[null,"PTX1"," 入出力"," MMC_CLK 出力 (MMCIF)"," －"," －"," －","USB0 Enable"]
[null,"PTX0"," 入出力"," MMC_CMD 入出力 (MMCIF)"," －"," －"," －","USB0 OverCurrent"]
[null,"PTY7"," 入出力"," SDHI0CD 入力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTY6"," 入出力"," SDHI0WP 入力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTY5"," 入出力"," SDHI0D3 入出力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTY4"," 入出力"," SDHI0D2 入出力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTY3"," 入出力"," SDHI0D1 入出力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTY2"," 入出力"," SDHI0D0 入出力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTY1"," 入出力"," SDHI0CMD 入出力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTY0"," 入出力"," SDHI0CLK 出力 (SDHI0)"," －"," －"," －","CAT724 microSD"]
[null,"PTZ7"," 入出力"," IRQ7 入力 (INTC)"," SCIF3_CTS 入力 (SCIFA3)"," －","PSB[10]/MSELB[5]","EB724では RS232C",4]
[null,"PTZ6"," 入出力"," IRQ6 入力 (INTC)"," SCIF3_RTS 出力 (SCIFA3)"," －","PSB[11]/MSELB[5]","EB724では RS232C",4]
[null,"PTZ5"," 入出力"," IRQ5 入力 (INTC)"," SCIF3_SCK 入出力 (SCIFA3)"," －","PSB[12]/MSELB[5]","CAT724 AX88796 割り込み"]
[null,"PTZ4"," 入出力"," IRQ4 入力 (INTC)"," SCIF3_RXD 入力 (SCIFA3)"," －","PSB[13]/MSELB[5]","EB724では RS232C",4]
[null,"PTZ3"," 入出力"," IRQ3 入力 (INTC)"," SCIF3_TXD 出力 (SCIFA3)"," －","PSB[14]/MSELB[5]","EB724では RS232C",4]
[null,"PTZ2"," 入出力"," IRQ2 入力 (INTC)"," －"," －"," －","EB724では未接続"]
[null,"PTZ1"," 入出力"," IRQ1 入力 (INTC)"," －"," －"," －","IRQ1 ユーザ使用可能割り込み"]
[null,"PTZ0"," 入出力"," IRQ0 入力 (INTC)"," －"," －"," －","IRQ0 ユーザ使用可能割り込み"]
[]
[null,null,"黄色の色掛けがデフォルトで選択されている機能"]
[null,null,"オレンジはEB724では設定変更不可能"]
[]
[{"$nulls":6},"個数"]
[null,null,"「GPIO使用可能」欄","1. EB724評価キットの外部端子CN2,CN7にでているのでそのままGPIOとして使用できる",null,null,52]
[null,null,null,"2. EB724評価キットの外部端子CN2,CN7にでているが、別な機能として使っているのでソフトウェアを変更すれば使用できる",null,null,12]
[null,null,null,"3. EB724評価キットでは未使用（未接続）なのでユーザ基板を作成すれば使用できる",null,null,18]
[null,null,null,"4. EB724評価キットでは別な機能として使っているのでユーザ基板を作成し、かつ機能変更（ソフト修正）すれば使用できる",null,null,47]
[]
[null,null,null,"ユーザ様が基板を作成する際、CAT724標準カーネル・ドライバを変更することなく、そのまま機能未割当ピンをGPIOとして使うには 1 と 3 を使ってください。",{"$nulls":4},70]
[null,null,null,"それでも不足する場合は 2 と 4 のピンをご検討ください。その際は カーネル、ドライバに何らかの修正が必要になります。",{"$nulls":4},129]